{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":159,"n_cols":7,"rows_kept":159,"cut":false,"hidden":false,"merged":[]}
["id","index","name","unit","min","max","prec"]
[4,100,"未定义","-",0,10,1]
[5,101,"大气温度","℃",-50,100,0.1]
[6,102,"大气湿度","%RH",0,100,0.1]
[7,103,"模拟气压","hPa",500,1500,0.1]
[8,104,"雨量","mm",0,100,0.1]
[9,105,"简易总辐射","W/m2",0,1500,1]
[10,106,"土壤温度","℃",-50,100,0.1]
[11,107,"土壤湿度","%",0,100,0.1]
[12,108,"风速","m/s",0,70,0.1]
[13,109,"风向","°",0,360,1]
[14,110,"蒸发","mm",0,1000,0.1]
[15,111,"雪量","mm",0,1000,0.1]
[16,112,"照度","Lux",0,200000,10]
[17,113,"日照时数","h",0,24,0.1]
[18,114,"光合","W/m2",0,2000,1]
[19,115,"雨量累计","mm",0,6000,0.1]
[20,116,"辐射累计","MJ/m2",0,1000,0.01]
[21,117,"有无雨雪",null,0,1,1]
[22,118,"噪声","dB",0,100,0.1]
[23,119,"水位","cm",0,10000,0.1]
[24,120,"二氧化碳","PPM",0,2000,1]
[25,121,"曝辐量","cal/cm2",0,3,1]
[26,122,"液位","mm",0,1000,0.1]
[27,123,"光合有效辐射","W/m2",0,2000,1]
[28,124,"电压","V",0,15,0.001]
[29,125,"紫外线","mW/m2",0,2000,1]
[30,126,"粉尘","ug/m3",0,4,0.1]
[31,127,"数字气压","hPa",10,1100,0.1]
[32,142,"电流","mA",0,5000,0.1]
[33,129,"最大风速","m/s",0,70,0.1]
[36,130,"平均风速","m/s",0,70,0.1]
[37,131,"经度","°",-180,180,0.1]
[38,132,"纬度","°",-90,90,0.1]
[39,133,"海拔高度","m",-2000,9000,0.1]
[40,134,"TBQ 总辐射","W/m2",0,2000,1]
[41,135,"直接辐射","W/m2",0,2000,1]
[42,136,"散射辐射","W/m2",0,2000,1]
[43,138,"紫外辐射","W/m2",0,2000,1]
[44,139,"贴片温度","℃",-50,100,0.1]
[45,140,"露点温度","℃",-50,40,0.1]
[46,141,"一氧化碳","PPM",0,1000,1]
[47,128,"pH 值",null,0,14,0.01]
[48,143,"超声波风速","m/s",0,60,0.01]
[49,144,"水温","℃",-50,100,0.1]
[50,145,"PM2.5","ug/m3",0,10,0.1]
[51,146,"PM10","ug/m3",0,10,0.1]
[52,152,"能见度","m",0,50000,0.1]
[53,147,0.1,null,0,10000,0.1]
[54,148,0.01,null,0,10000,0.01]
[55,149,0.001,null,0,10000,0.001]
[56,150,"PM2.5","ug/m3",0,2000,1]
[57,151,"PM10","ug/m3",0,2000,1]
[58,153,"负氧离子","个/cm3",0,5000,10]
[59,154,"盐分","mg/L",0,15000,1]
[60,155,"电导率","mS/cm",0,20,0.01]
[61,156,"SO2","ug/m3",0,20000,1]
[62,157,"CO","mg/m3",0,2000,0.01]
[63,158,"NO2","ug/m3",0,2000,1]
[64,159,"O3","ug/m3",0,2000,1]
[65,160,"管道流量","m3/s",0,1000,0.01]
[66,161,"流速","L/min",0,10000,1]
[67,162,"管道压力","KPa",0,10000,1]
[68,163,"温差","℃",-150,150,0.1]
[69,164,"溶解氧","mg/L",0,20,0.01]
[70,165,"溶解氧差","mg/L",-20,20,0.01]
[71,166,"氨氮","mg/L",0,2000,0.1]
[72,167,"负氧离子","个/cm3",0,50000,1]
[73,168,"TSP","ug/m3",0,2000,1]
[74,169,"水位","m",0,300,0.01]
[75,170,"浊度","NTU",0,20,0.1]
[76,171,0.016,null,0,1000,0.016]
[77,172,0.019,null,0,1000,0.019]
[78,173,0.2,null,0,1000,0.2]
[79,174,0.3,null,0,1000,0.3]
[80,175,0.5,null,0,1000,0.5]
[81,176,0.7,null,0,1000,0.7]
[82,177,0.8,null,0,1000,0.8]
[83,178,0.9,null,0,1000,0.9]
[84,179,0.022,null,0,1000,0.022]
[85,180,0.025,null,0,1000,0.025]
[86,181,"SO2","ppb",0,20000,1]
[87,182,"CO","ppb",0,20000,1]
[88,183,"NO2","ppb",0,20000,1]
[89,184,"O3","ppb",0,20000,1]
[90,185,"NH3","ppm",0,5000,0.01]
[91,186,"H2S","ppm",0,5000,0.01]
[92,187,"氧气","%Vol",0,1000,0.1]
[93,188,"声波液位","mm",0,30000,0.4]
[94,189,"5min-PM25","ug/m3",0,2000,1]
[95,191,"水位","m",0,10000,0.1]
[96,190,"5min-PM10","ug/m3",0,2000,1]
[97,192,"归零",0,0,0,0]
[98,193,"CO","mg/m3",0,2000,0.1]
[99,194,"CH4","%LEL",0,100,0.1]
[100,195,"CH4S","mg/m3",0,2000,0.001]
[101,196,"能见度","m",0,60000,1]
[102,197,0.105,"℃",-500,10000,0.105]
[103,198,"土壤盐分",null,0,10000,1]
[104,199,"累积流量","m3",0,60000,0.01]
[105,200,"菌落总数","CFU",0,800,1]
[106,201,"土壤热通量","w/m2",-500,500,0.1]
[107,202,"液位","mm",0,5000,1]
[108,203,"液位","mm",0,20000,1]
[109,204,"氨氮","ppm",0,300,0.1]
[110,205,"1.2PM","ug",0,1000,1.2]
[111,206,"1.5PM","ug",0,1000,1.5]
[112,207,"毫米汞柱","mmHg",0,2000,0.1]
[113,208,"照度","Lux",0,200000,1]
[114,209,"电压","V",0,100000,0.1]
[115,210,"电流","A",0,100000,0.1]
[116,211,"ORP","mV",-10000,10000,0.01]
[117,212,"电压","V",0,10000,1]
[118,213,"电流","A",0,10000,1]
[119,214,"电量","KW·h",0,10000,0.01]
[120,215,"流量","m3/h",0,10000,0.01]
[121,216,"累计流量","m3",0,30000,1]
[122,217,"累计流量","L",0,30000,1]
[123,218,"编码",null,0,20000,1]
[124,219,1,null,0,30000,1]
[125,220,"电导率","uS/cm",0,30000,1]
[126,221,"路面状况",null,0,100,1]
[127,222,"直径","mm",0,30000,0.1]
[128,223,100,null,0,30000,100]
[129,224,1000,null,0,30000,1000]
[130,225,"流量","m3/h",0,30000,0.1]
[131,226,"ppm","ppm",0,30000,0.001]
[132,227,10,null,0,30000,10]
[133,228,"湿度","%RH",0,100,0.001]
[134,229,"辐射","W/m2",0,30000,1]
[135,230,0.0001,null,0,30000,0.0001]
[136,231,1e-5,null,0,30000,1e-5]
[137,232,1e-6,null,0,30000,1e-6]
[138,233,0.001,"m/s",0,10000,0.001]
[139,234,0.1,"m3",0,10000,0.1]
[140,235,0.001,"m3/s",0,10000,0.001]
[141,236,"0.1 风向","°",0,360,0.1]
[142,237,"0.01 大气温度","℃",0,100,0.01]
[143,238,"0.01 大气湿度","%RH",0,100,0.01]
[144,239,"氮离子","mg/KG",0,500,1]
[145,240,"钾离子","mg/KG",0,500,1]
[146,241,"磷离子","mg/KG",0,500,1]
[147,242,0.0001,null,0,30000,0.0001]
[148,243,1e-5,null,0,30000,1e-5]
[149,244,"流量","mL",0,30000,1]
[150,245,"流速","mL/s",0,30000,1]
[151,246,"重量","g",0,30000,1]
[152,247,"百分比","%",0,30000,0.01]
[153,248,"分米","dm",0,30000,0.01]
[154,249,"模式",null,0,30000,1]
[155,250,"电机",null,0,30000,1]
[156,251,"方向",null,0,30000,1]
[157,252,"开关状态",null,0,30000,1]
[158,253,"PAR","W/m2",0,30000,0.01]
[159,254,"PPFD","umol/m2/s",0,30000,0.1]
[160,255,"YPFD","umol/m2/s",0,30000,0.1]
[161,256,"辐射","W/m2",0,30000,0.01]
[162,257,"色温","K",0,30000,1]
[163,258,"辐照度","mW/m2",0,30000,0.01]